A B C D E F G H I K L M N O P Q R S T U V W

## C

CancelChineseCharModel() - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
cancelChineseCharModel() - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
CancelChineseCharModel() - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
cancelUserDefinedCharacters(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
cancelUserDefinedCharacters(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
cancelUserDefinedCharacters(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Cancel user-defined characters Cancel user-defined characters with code n
cancelUserDefinedChineseChar(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
canclePrintDataByPagemodel() - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Cancel printing data in page mode
checkLableAndGap() - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
CheckLinkedState(TaskCallback) - Method in interface net.posprinter.posprinterface.IMyBinder
  Check linked state
checkLinkedState(String, TaskCallback) - Method in interface net.posprinter.posprinterface.PrinterBinder
CheckLinkedState(TaskCallback) - Method in class net.posprinter.service.PosprinterService.MyBinder
checkLinkedState(String, TaskCallback) - Method in class net.posprinter.service.PrinterConnectionsService.printerBinder
checkPrinterStateByPort4000() - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command is used on port 4000, once sent, the printer will return the data representing the status once
checkPrinterStateByPort9100() - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command obtains the printer status at any time, even in the event of printer error.
clear() - Method in class net.posprinter.utils.RoundQueue
ClearBuffer() - Method in interface net.posprinter.posprinterface.IMyBinder
  Clear buffer
clearBuffer(String) - Method in interface net.posprinter.posprinterface.PrinterBinder
ClearBuffer() - Method in class net.posprinter.service.PosprinterService.MyBinder
clearBuffer(String) - Method in class net.posprinter.service.PrinterConnectionsService.printerBinder
Close() - Method in class net.posprinter.utils.PosPrinterDev
cls() - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command clears printer buffer.
codeBlockFMode(int, int, int, int, int, String) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command draws CODABLOCK F mode barcode.
codePage(String) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command is used to define the international character set corresponding to each letter key of the portable keyboard (optional, KP-200)
compressBmpByPrinterWidth(Bitmap, BitmapProcess.PrinterWidth) - Static method in class net.posprinter.utils.BitmapProcess
  Compress the picture according to the width of the printing paper
compressBmpByYourWidth(Bitmap, int) - Static method in class net.posprinter.utils.BitmapProcess
  Compress the picture according to the width you give.
ConnectBtPort(String, TaskCallback) - Method in interface net.posprinter.posprinterface.IMyBinder
  Connect printer by bluetooth
connectBtPort(String, TaskCallback) - Method in interface net.posprinter.posprinterface.PrinterBinder
ConnectBtPort(String, TaskCallback) - Method in class net.posprinter.service.PosprinterService.MyBinder
  Connect printer by bluetooth
connectBtPort(String, TaskCallback) - Method in class net.posprinter.service.PrinterConnectionsService.printerBinder
ConnectNetPort(String, int, TaskCallback) - Method in interface net.posprinter.posprinterface.IMyBinder
  Connect printer by network port
connectNetPort(String, TaskCallback) - Method in interface net.posprinter.posprinterface.PrinterBinder
ConnectNetPort(String, int, TaskCallback) - Method in class net.posprinter.service.PosprinterService.MyBinder
  Connect printer by wifi
connectNetPort(String, TaskCallback) - Method in class net.posprinter.service.PrinterConnectionsService.printerBinder
ConnectUsbPort(Context, String, TaskCallback) - Method in interface net.posprinter.posprinterface.IMyBinder
  Connect printer by usb
connectUsbPort(Context, String, TaskCallback) - Method in interface net.posprinter.posprinterface.PrinterBinder
ConnectUsbPort(Context, String, TaskCallback) - Method in class net.posprinter.service.PosprinterService.MyBinder
  Connect printer by usb
connectUsbPort(Context, String, TaskCallback) - Method in class net.posprinter.service.PrinterConnectionsService.printerBinder
country(String) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command orients the keyboard for use in different countries via defining special characters on the KP-200 series portable LCD keyboard (option).
creatCashboxContorlPulse(int, int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
creatCashboxContorlPulse(int, int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
creatCashboxContorlPulse(int, int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Generate cash drawer control pulse
cut() - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command activates the cutter to immediately cut the labels without back feeding the label.
cutBitmap(int, Bitmap) - Static method in class net.posprinter.utils.BitmapProcess
  Cutting picture method, cutting picture with equal height, return to List

A B C D E F G H I K L M N O P Q R S T U V W